|  |  |
| --- | --- |
| BR 952 005 | ClassicLine tank eyewash station with 60-litre-tank, wall-/table mounted |
| ClassicLine tank eyewash station with 60-litre-tank, wall-/table mounted  - for mobile use or when no water connection is available  - tank of chemical-resistant plastic, green, with a tank capacity of 60 litres  - tank is sufficient for approx. 15 minutes uninterrupted flushing time  - water inlet via large screw cap, top of tank  - easy and simple activation by dragging down the pull strip  - softly radiating low-pressure spray heads, which supply both eyes with the rinsing liquid  - sign for eye shower according to DIN EN ISO 7010 und ASR A1.3, self-adhesive PVC-film, 100 x 100 mm, viewing distance 10 metre  - dimensions (H x W x D): 580 x 450 x 450 mm  - according to ANSI Z358.1-2014 and DIN EN 15154-4:2009 Manufacturer: B-SAFETY or equal Article-No.: BR 952 005  **Technical Specifications**  Material: GFK-plastic, chemical resistant  Color: green  Dimensions (H x W): 580 x 450 mm  Tank capacity: 60 litre  Flush time: about 15 minutes  Water filling: screw cap | |