|  |  |
| --- | --- |
| BR 952 005 | ClassicLine tank eyewash station with 60-litre-tank, wall-/table mounted |
| ClassicLine tank eyewash station with 60-litre-tank, wall-/table mounted- for mobile use or when no water connection is available- tank of chemical-resistant plastic, green, with a tank capacity of 60 litres- tank is sufficient for approx. 15 minutes uninterrupted flushing time- water inlet via large screw cap, top of tank- easy and simple activation by dragging down the pull strip- softly radiating low-pressure spray heads, which supply both eyes with the rinsing liquid- sign for eye shower according to DIN EN ISO 7010 und ASR A1.3, self-adhesive PVC-film, 100 x 100 mm, viewing distance 10 metre- dimensions (H x W x D): 580 x 450 x 450 mm- according to ANSI Z358.1-2014 and DIN EN 15154-4:2009Manufacturer: B-SAFETY or equalArticle-No.: BR 952 005**Technical Specifications**Material: GFK-plastic, chemical resistantColor: greenDimensions (H x W): 580 x 450 mmTank capacity: 60 litreFlush time: about 15 minutesWater filling: screw cap |