|  |  |
| --- | --- |
| BR 960 005 | ClassicLine mobile tank eyewash station with stainless steel tank |
| ClassicLine mobile tank eyewash station with stainless steel tank  - tank of stainless steel, with a capacity of 16 litres, on handcart with solid rubber tyres  - water inlet via large flap lid on the tank, compressed air connection tyre inflation valve  - for mobile use or when no water connection is available  - actuation by activation of the hand-held eye shower  - hand-held eye shower with one spray head, mounting by wall bracket on the tank  - ergonomically shaped handle with integrated, adjusting activation made of plastics, valve not self-closing  - aerators made of brass with a very limited spray pattern, chrome-plated  - integrated automatic flow regulator 7 litres / minute (1.7 litres / minute / 0.45 GPM) for a standard-compliant spray pattern  - integrated backflow preventer  - stainless steel covered hose, length 1.5 meter, water inlet ½” female, DIN-DVGW tested and certificated  - sign for eye shower according to DIN EN ISO 7010 und ASR A1.3 mounted on the tank, self-adhesive PVC-film, 150 x 150 mm, viewing distance 15 metre  - dimensions (H x W x D): 850 x 450 x 225 mm  - according to ANSI Z358.1-2014 Manufacturer: B-SAFETY or equal Article-No.: BR 960 005  **Technical Specifications**  Dimensions (H x W): 850 x 450 mm  Filling volume: 14 litre  Filling pressure: 7 bar  Flow rates: 7 l/min / 1.7 l/min (0.45 GPM)  Flush times: about 2 minutes / 5 minutes  Water filling: flap lid  Compressed air connection: tyre inflation valve  **Product Overview**  BR 960 005: flow rate 7 l/min, flush time about 2 minutes  BR 960 005 / 1L: flow rate 1.7 l/min (0.45 GPM), flush time about 5 minutes | |